Multistage, non-self-priming, horizontal high-pressure centrifugal pump in block design with horizontal suction- and vertical pressure port.

The pump has a compact design with a continuous motor pump shaft and a bidirectional mechanical seal.

The pump is suitable for water supply and pressure boosting, industrial recirculation systems, process water and closed cooling circuits. It can also be used in washing systems, irrigation as well as for water treatment.

Special features/product advantages

 Space-saving, compact block design
 All hydraulic parts which come into contact with the fluid, such as stage chambers, impellers and diffusors and the pump housing are made of stainless steel
 Drinking water approval (ACS, KTW, WRAS) for all components in contact with the fluid (EPDM version)

Scope of delivery

 Wilo-Economy MHI high-pressure multistage centrifugal pump
 Installation and operating instructions

Design notes

 Motor protection for three-phase AC motor is optional or to be provided on-site
 Single-phase AC motor equipped with built-in thermal motor protection and capacitor

Материалы

Рабочее колесо: 1.4301 [AISI304]
Корпус насоса: 1.4301 [AISI304]
Вал насоса: 1.4301 [AISI304]
Статическое уплотнение: EPDM
Mechanical seal: BQ1E3GG

Мощность

Температура перекачиваемой жидкости T: -15...+110 °C
Температура окружающей среды, макс. T: 40 °C
Входное давление      макс. H: 6 бар

Мотор

Класс изоляции: F
Степень защиты: IP 54
Подключение к сети: 3~400 В, 50 Гц
Номинальная мощность электродвигателя P2: 1.10 кВт
Потребляемая мощность P1: 1.58 кВт
Номинальный ток 3~230 В, 50 Гц IN: 4.8 A
Номинальный ток 3~400 В, 50 Гц IN: 2.8 A
КПД электродвигателя ηm 50% : 81,5 %
КПД электродвигателя ηm 75% : 82,7 %
КПД электродвигателя ηm 100% : 82,7 %

Подключения

Номинальный внутренний диаметр патрубков на стороне всасывания Rp: 1½
Номинальный внутренний диаметр патрубков с напорной стороны Rp: 1¼

Данные для заказа

Изделие: Wilo
Тип: MHI 803
Арт.-№: 4210743
Вес, прим. m: 13.1 кг